PANASONIC WV-X5550LT VEHICLE CAPTURE CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	Panasonic i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	PANASONIC WV-X5550LT VEHICLE CAPTURE CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Vehicle Capture Camera shall deliver H.265 stream and H.264 stream. 

2.	The Vehicle Capture Camera shall produce a resolution of  2560 x 1920 pixels at up to
 30 fps in single source with a 4:3 aspect ratio. 

3.	The Vehicle Capture Camera shall utilize an approximate 2/3 type high sensitivity CMOS image sensor. 

4.	The Vehicle Capture Camera shall equipped dual source capturing function for enables to capture clear occupant and license plate images simultaneously.

5.	The Vehicle Capture Camera shall equipped a high powered IR floodlight with 78 LEDs light arrays  to produce a clear monochrome capture image in zero lux conditions with 21 - 26 meters  (69 to 86 feet) irradiation distance.

6.	The Vehicle Capture Camera shall built-in Polarized Filter to cut through reflections to capture occupant even with curved windshield at day time.

7.	The Vehicle Capture Camera shall adapted special Band-Pass Filter for even in intense headlights, the flare is suppressed and occupant can be captured clearly at night time.

8.	The Vehicle Capture Camera shall switched between two types of optical filters (Polarized Filter / Band-Pass Filter) to captures clear occupant’s images in all day.

9.	The Vehicle Capture Camera shall feature a 120dB multi-sampling dynamic range and 
Adaptive Black Stretch technology (ABS). 
        Multi-sampling dynamic range shows the maximum exposure ratio of source 1 which is
driver's face image and source 2 which is license plate image.

10.	The Vehicle Capture Camera shall generate two simultaneous video streams of H.265 (Main profile) or H.264 (High profile) stream and JPEG stream.

11.	The Vehicle Capture Camera shall built-in motorized optical zoom up to 1.7 times and motorized focus for easy adjustment at installation.

12.	The Vehicle Capture Camera shall be equipped with intelligent auto mode, the technology for shooting license plate and occupant more clearly
                                                                                         
13.	The Vehicle Capture Camera shall produce encrypted stream.

14.	The Vehicle Capture Camera shall be rated to IK10 vandal resistance.

15.	The Vehicle Capture Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress.

16.	A user shall be able to view video on a PC using a browser.

17.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

18.	The Vehicle Capture Camera shall have High light compensation (HLC) function.

19.	The Vehicle Capture Camera shall have a USB terminal for confirming the live image and adjusting viewing angle with the smartphone or tablet device via the Wi-Fi connection at installation. 

B.	CAMERA
1.	Image Sensor		2/3 type CMOS image sensor
2.	Effective Pixels                  Approx. 5.1 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	B/W			0.0 lux (with IR LED on)
5.	Dynamic Range		120 dB typ. (Multi-sampling dynamic range)
6.	Built-in IR illumination
a.	Irradiation distance	Approx. 21 - 26 meters  (69 to 86 feet)

C.	Lens
1.	Vari-Focal Length		51 ~ 85mm (2-9/16 ~ 3-11/32 inches)
2.	Max. Aperture Ratio	1 : 1.6
3.	Angular Field of View
a.	4:3 aspect ratio	H: 5.5° (TELE) - 9.2° (WIDE)
V: 4.4° (TELE) - 7.3° (WIDE)
4.	Adjusting Angle                 
                                          Horizontal (PAN) angle: ±17°
                                          (can be adjusted with the installation angle of the TILT bracket)
Vertical    (TILT) angle: ±10°

5.	Focus Adjustment		Motorized
6.	Optical Zoom Ratio           1.7x (Motorized)

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	4:3 aspect ratio 
(H.265/H.264) 2560x1920, 1600x1200, 1280x960, 640x480 
(JPEG)           1280x960, 640x480 
3.	H.265 / H.264
a.	Transmission Mode	VBR / Frame rate
b.	Frame Rate		(30fps mode) 1 / 3 / 7.5 / 10 /15 / 30 fps
                                  (25fps mode) 1 / 3.1 / 6.25 / 8.3 /12.5 / 25 fps
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1,024 / 1,536 / 2,048 / 3,072 / 
4,096 / 6,144 / 8,192 / 10,240 / 12,288 / 14,336 / 16,384 / 20,480 / 24,576 kbps
d.	Image Quality	
i.	Frame rate            Motion priority / Normal / Quality priority
ii.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast

4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push

E.	OPERATION
1.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
2.	Back light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
The level can be set in the range of 0 to 31.
(only when Intelligent Auto : Off) 
3.	Shutter Speed		1/10000 to 1/30 s (15fps/30fps mode)
                                          1/10000 to 1/25 s (12.5fps/25fps mode) 
4.	Day & Night		Auto*/ Day/ Night   *The level can be set in the range of 0 to 9.
5.	Digital Noise Reduction	The level can be set in the range of 0 to 255.

F.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, DNS, NTP, DHCPv6, RTP,
MLD, ICMP, ARP
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP,
DHCP, DNS, NTP, IGMP, ICMP, ARP
4.	Max. User access		Up to 14 users(Number of sessions that can connect to cameras   
     at the same time)     *Depends on network conditions
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals
G.	INTERFACE
1.	Monitor Output		USB terminal via Wi-Fi connection

H.	ELECTRICAL
1.	Power Source		AC24 V 3.8 A
2.	Power Consumption	Approx.  68W

I.	SAFETY / EMC
1.	Safety			UL (UL62368-1), c-UL (CAN/CSA C22.2 NO.62368-1),
 CE (EN62368-1)
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class A, 
				EN55024

J.	MECHANICAL
1.	Dimensions 		Ceiling mount
303 mm (W) x 475 mm (H) x 368 mm (L) 
{11-15/16 inches (W) x 18-11/16 inches (H) x 14-1/2 inches (L)} 
Pole mount
303 mm (W) x 396 mm (H) x 458 mm (L) 
{11-15/16 inches (W) x 15-19/32 inches (H) x 18-1/32 inches (L)}
Stationary mount
303 mm (W) x 440 mm (H) x 368 mm (L) 
{11-15/16 inches (W) x 17-5/16 inches (H) x 14-1/2 inches (L)}

2.	Weight			Approx. 11.5 kg {25.39 lbs}
                                          Approx. 16.0 kg {35.32 lbs}   With TILT bracket  

3.	Construction material
a.	Main body		Aluminum die cast
Glass and Polycarbonate resin
b.	Outer fixing screws   Stemless steel (Corrosion-resistant treatment)
c.	TILT bracket		Aluminum plate and Aluminum die cast
4.	Finish
a.	Main body		Silver
		Clear

K.	ENVIRONMENTAL
1.	Ingress Resistance	IP66 (IEC60529), Type 4X (UL50E), NEMA 4X compliant, 
2.	Vandal Resistance	IK10 (IEC 62262)
3.	Wind Resistance               Up to 40 m/s {approx. 89 mph}
4.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F,)
 (Power On range : –20 °C to +60 °C {–4 °F to +140 °F})
5.	Operating Humidity	 10 % ~ 100 % (without condensation)