i-PRO Server based recording and video management platform
WV-ASR500 Series

DIVISION 28 – ELECTRONIC SAFETY AND SECURITY

28 20 00 ELECTRONIC SURVEILLANCE

28 23 00 Video Surveillance

28 23 13 Video Surveillance Control and Management Systems

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Note to Specifier:  This guide specification incorporates CSI MasterFormat™ 2004 Edition Numbers and Titles.

(Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.)

PART 1  GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2  PRODUCTS

2.01	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd 

B.	Provide i-Pro camera Open platform and high performance Server based recording and video management platform

2.02	i-Pro Server based recording and video management platform

A.	The WV-ASR500 Series shall support following key features:
	- Open platform, i-PRO's and 51 other vendor's network cameras support.
	- Up to 64 network cameras can be connected and recorded.
	- Up to 16 clients can monitor image and control WV-ASR500 simultaneously. 
	   (Depends on system structure, environment.)
	- Various Recording Modes: Schedule, Event (Pre/Post)
	- Graphical Timeline Search function (with WV-ASC970 System)
	- H.264, MPEG-4 and JPEG multi format
	- Cooperative with the Face Matching System (WV-ASF900 Series)
	- Supports archiving function to realize long-term recording (as of March 2014)
	- Can be linked with Electric Access Control and POS System (as of March 2014)

B.	Supported Cameras: 
(1)	Compatible vendor: 51 Vendors , Onvif compliant models
(2)	Supported Image Format: H.264, MPEG-4, M-JPEG
(3)	Supported Image Resolution: Up to 1920×1080, 2048×1536
(4)	Maximum Number of Cameras: MAX. 64

C.	Recording:
(1)	Recording Mode: Schedule including Event (Pre/Post)
(2)	Pre-Event Recording: Up to 120 seconds
(3)	Scheduled Recording Mode: Motion / Free run / Alarm
(4)	Frame Rate/Camera: Up to 30ips (Depending on the Camera)
(5)	RAID Configuration: RAID-5

D.	Alarm / Event:
(1)	Alarm Source: VMD, Event Linking
(2)	Alarm Action: Record Video, Output trigger, Pan/tilt/zoom preset, e-mail notification, Auto export

E.	Network:
(1)	Network Interface: Network Interface
(2)	E-mail: Upon Alarm

F.	OS:
(1)	Microsoft® Windows® Server 2012 Standard

G.	Channel License per server:
(1)	1ch: WV-ASRE501
(2)	16ch: WV-ASRE516
(3)	32ch: WV-ASRE532
(4)	64ch: WV-ASRE564

H.	Different Items of “WV-ASC970/ASM970 with ASR500”:GUI difference compared with NDR (as of Nov, 2013):
- Video display monitor control
	Audio Trans. On/Off: The sending side does not work.
	Audio Recep. On/Off: The receiving does not work.
	OSD On/Off: The live video is displayed via ASR500, in playback, OSD is not displayed.
	EL-Zoom: It dose not work.
	Optical Zoomx1: It dose not work at equally times zoom
	Click & Centering: Click & Centering dose not work.
	Drag & Zoom: Drag & Zoom dose not work.
        - Camera control panel
	Camera Control: In camera control via ASR500, Pan, Tilt, Zoom, Preset Move, 
		Preset Set regarding above only, it will work.
        - Device Web screen display from camera tree
	Operating Window: It cannot boot ASR500 Web browser screen.
                                    (“Operating Window” character line will be gray out)
        - Playback panel (InstantPlayback/SyncPlayback)
	Time line type addition: “Event Linking” recording type will be added.
	Double-speed playback: Up to step 5. *Even if the user specify STEP6, STEP7, it will  
                                                      playback by STEP5
	Playback method: For ASR500, ASM970 needs to download records during playback.
                                     *It takes time to start playback.
                                     *When ASM970 reaches the end of downloaded records, ASM970
                                        start to download again to play back continuously.
        - Recording data search screen
	addition of Event: As event type, “Event Linking” is added.
	Search target event: Available recording event types are Schedule, VMD and Event.
        - The screen of recording data search result
	Audio icon: The audio icon is not displayed in the list for search result
	Download: The file will be AVI: It can playback by Windows Media Player.
        - Download panel
	Download: The file is AVI. It can playback by Windows Media Player.
	                        Also even if the audio check box is checked, the video with audio 
	                        data cannot be downloaded.
        - Alarm history search
	Search target alarm type: Against ASR500, Motion(cam),  I/O Port,  Capacity Warm(dvr), 
			 and Comm Err(cam): alarm-occur history is displayed as search result.

PART 3  EXECUTION

3.01	ACCEPTABLE INSTALLERS
3.01	INSTALLATION