i-PRO Model WJ-GXE100 H.264 Network Video Encoder

DIVISION 28 – ELECTRONIC SAFETY AND SECURITY

28 20 00 ELECTRONIC SURVEILLANCE

28 23 00 Video Surveillance

28 23 29 Video Surveillance Remote Devices and Sensors

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Note to Specifier:  This guide specification incorporates CSI MasterFormat™ 2004 Edition Numbers and Titles.

(Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.)

PART 1  GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2  PRODUCTS

2.01	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd.

B.	Provide Single-channel Video Encoder from single source manufacturer.

2.02	One Channel Video Server / Video Encoder

A.	The one channel video encoder shall be a i-PRO Model WJ-GXE100 or equivalent.  

B.	The video encoder shall convert analog video signals to digital data (MJPEG or H.264). 

C.	The encoder shall distribute MJPEG/H.264 through the network with minimal image degradation.

D.	The encoder shall support 3 streams simultaneously combined MJPEG and H.264 Video Compression.

E.	The encoder shall generate and transmit images to meet the following Resolutions: 

Picture (Camera) mode:	VGA [4:3]
H.264  VGA (640x480)/QVGA (320x240), max. 30 fps
JPEG  VGA (640x480)/QVGA (320x240), max. 30 fps

Picture (Camera) mode: 	VGA [16:9]
H.264  VGA (640x360)/QVGA (320x180), max. 30 fps
JPEG  VGA (640x360)/QVGA (320x180), max. 30 fps

Picture (Camera) mode:	D1
H.264  D1 (720x480), max. 30 fps
JPEG  D1 (720x480), max. 30 fps

F.	The encoder shall be able to support 30 fps per channel.

G.	The encoder shall connect 1 analog camera and control its functions such as Pan/tilt/zoom, focus, preset positions, auto focus and brightness remotely.

H.	The encoder shall feature Video motion detection.

I.	The encoder shall feature a camera title of 20 alphanumeric characters (or marks). 

J.	The encoder shall support 10BASE-T/100BASE-TX.

K.	The encoder shall be able to support unicast and multicast transmissions.

L.	The Max bit rate per client for H.264 shall be selectable from 64 kbps/ 128 kbps/ 256 kbps/ 384 kbps/ 512 kbps/768 kbps/ 1024 kbps/ 1536 kbps/ 2048 kbps/ 3072 kbps/4096 kbps and combined with Bandwidth control (Unlimited/ 64 kbps/ 128 kbps/ 256 kbps/ 384 kbps/512 kbps/ 768 kbps/ 1024 kbps/ 2048 kbps/ 4096 kbps/8192 kbps ). 

M.	Supported protocols: IPv6: TCP/IP, UDP/IP, HTTP, HTTPS, RTP, FTP, SMTP, DNS, NTP, SNMP, DHCPv6, MLD, ICMPv6 and IPv4: TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, FTP, SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP, ARP.

N.	The encoder shall support the scheduled transfer of image data via FTP to an FTP server. 

O.	The encoder shall have a built in web server so that access to the IP video stream can be obtained using Internet Explorer Version 7.0 or later.   The web browser shall permit the user to make adjustments and settings to the encoder.

P.	The encoder shall be able to control PTZ cameras and automatically sequence through the preset positions in logical programming order (sequence mode) or actual position (sort mode). 

Q.	The encoder shall protect all menu settings on web pages with user-id and password.

R.	The encoder shall provide the ability to display multiscreen of 4 encoders/cameras as a group and up to 4 groups (16 cameras) to be registered.

S.	The encoder shall permit a physical, external time adjustment input or time adjustment via external, user-supplied NTP server.

T.	The camera shall support SSL mail server (only with “Gmail”).

U.	The camera shall have HTTP Alarm notification function in setup menu.

V.	The camera shall have Advanced VBR in transmission priority.

W.	The camera shall be compliant with ONVIF.

X.	The power source shall be 12V DC @ 200mA or PoE IEEE 802.3af (PoE 48 V: 75mA) compliant power device. 

Y.	All units shall be UL listed.

PART 3  EXECUTION

3.01	ACCEPTABLE INSTALLERS
3.01	INSTALLATION