i-PRO WJ-PC200/WJ-PC200E Coaxial - LAN Converter Receiver side unit
i-PRO WJ-PR201/WJ-PR201E Coaxial - LAN Converter Camera side unit
i-PRO WJ-PR204/WJ-PR204E Coaxial - LAN Converter Camera side unit
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormat™ 2004 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer.

2.2	i-PRO WJ-PC200 / WJ-PC200E, WJ-PR201 / WJ-PR201E, WJ-PR204 / WJ-PR204E Coaxial - LAN Converter

A.	GENERAL CHARACTERISTICS
1.	The Coaxial-LAN Converter shall be configured the camera side and the receiver side.

2.	The Coaxial-LAN Converter shall be compliant with PoE standards and contain a power supplying device. 

3.	Then Coaxial-LAN Converter shall be used at the distance of 500m (1,640 feet) with 5C-2V or RG-6/U coaxial cable with Poe power supply to camera.

4.	The Coaxial-LAN Converter shall be used at the distance of up to 2,000m (6,560 feet) with external power supply. 

5.	The Coaxial-LAN Converter shall be capable of transmission speed of 35 Mbps or over, when using TCP.

6.	The Coaxial-LAN Converter shall be capable of transmission speed of 45 Mbps or over, when using UDP. 

7.	[WJ-PR204]
The Coaxial-LAN Converter shall connect up to 4 network cameras on a single receiver side. 

B.	PERFORMANCE
1.	Number of connected camera
a.	WJ-PR204		Up to 4 cameras
b.	WJ-PR201		1 camera
2.	Maximum number of Devices
128 units in 1 segment
3.	Transmission Speed
a.	UDP			45 Mbps or higher 
b.	TCP 			35 Mbps or higher
4.	Maximum Transmission Distance of a Coaxial Cable
a.	Without PoE		2.0 km (6, 540 feet, when using WJ-PR201)
b.	With PoE		500 m (1,640 feet, when using a i-PRO network camera)
300 m (984 feet, when using a Class0 standard network camera)
c.	With PoE+		300 m (984 feet, when using a i-PRO network camera)
200 m (656 feet, when using a Class4 standard network camera)

C.	Coaxial INTERFACE
1.	Frequency Range		2 MHz - 2.8 MHz
2.	Data Transfer Mode	Wavelet OFDM
3.	Access Method		CSMA / CA
4.	Error Correction		Reed-Solomon Code + Convolutional Code (Viterbi decoding)

D.	NETWORK
1.	Standard			IEEE802.3 / IEEE802.3u
2.	MDI / MDI-X		Cross / Straight cable automatic recognition
3.	Number of port		1 (RJ45 connector)
4.	Protocols			TCP/IP, UDP
5.	Access Method		CSMA / CD

E.	ELECTRICAL
1.	Power Source		
a.	WJ-PC200		via Receiver unit
b.	WJ-PR201/WJ-PR204
			DC57V, AC 24V, PoE (Class 0)
2.	Power Consumption	
a.	WJ-PR201		Approx. 40W (DC 57V), Approx. 12.95W (PoE)
b.	WJ-PR204		Approx. 64W (DC 57V), Approx. 12.95W (PoE)

F.	MECHANICAL
1.	Dimensions (D x H)	
a.	WJ-PC200		76 mm x 76 mm x 36 mm ( 3 x 3 x 1-7/16 inches) 
(Excluding BNC connector cover)
b.	WJ-PR201/WJ-PR204
105 mm x 44 mm x 98 mm (4-5/32 x 1-3/4 x 6-1/2 inches)
			   (Excluding BNC connector cover)
2.	Weight			
a.	WJ-PC200		Approx. 110 g (0.24 lbs.)
b.	WJ-PR201		Approx. 250 g (0.55 lbs)
c.	WJ-PR204		Approx. 270 g (0.6 lbs)
3.	Construction material	
a.	WJ-PC200		PC/ABS resin
4.	Finish
a.	WJ-PC200		Sail white
b.	WJ-PR201/WJ-PR204
Silver

G.	ENVIRONMENTAL
1.	Operating Temperature	
a.	WJ-PC200		-10 °C ~ +50 °C (+14 °F ~ 122 °F)
b.	WJ-PR201/WJ-PR204
0 °C ~ +50 °C (+32 °F ~ 122 °F)
2.	Operating Humidity	 10 % ~ 90 % (without condensation)