PANASONIC WV-S8530N MULTI-SENSOR NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE

28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of Panasonic Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	Panasonic i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	PANASONIC WV-S8530N MULTI-SENSOR NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Multi-Sensor Camera shall deliver H.265 stream and H.264 stream.

2.	The Multi-Sensor Camera shall utilize an approximate 1/3 type high sensitivity CMOS image sensor. 

3.	The Multi-Sensor Camera shall have four FHD image sensors and produce a resolution of 1,920 x 1,080 pixels at up to 30 fps with a 16:9 aspect ratio. 

4.	The Multi-Sensor Camera shall have four FHD image sensors and produce a resolution of 1,600 x 1,200 pixels at 30fps with a 4:3 aspect ratio. 

5.	The Multi-Sensor Camera shall have the four repositionable lenses with easy adjustment include a wide range tilt angle (+ 80 degrees to 0 degree(right below) to  -15 degrees) mechanism minimizes blind spots. 

6.	The Multi-Sensor Camera shall be equipped with 1.8 times optical zoom at FHD resolution. 

7.	The Multi-Sensor Camera shall feature a 108dB wide dynamic range based on Enhanced Super Dynamic and Adaptive Black Stretch technology (ABS). 

8.	The Multi-Sensor Camera shall produce a color image with a minimum illumination of 0.09 lux and a monochrome image with 0.04 lux(F2.2, shutter speed : 1/30s, AGC : 11). 

9.	The Multi-Sensor Camera shall be equipped with a special coated cover for increasing the operational utility of outdoor cameras in rain weather.

10.	The Multi-Sensor Camera shall generate multiple simultaneous video streams of up to two (2) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams per camera.

11.	The Multi-Sensor Camera shall be equipped with intelligent auto mode, the technology for shooting license plate more clearly.

12.	The Multi-Sensor Camera shall be equipped with GOP control which has five selectable control modes (including frame rate control) for longer recording and less storage.

13.	The Multi-Sensor Camera shall produce encrypted stream.

14.	The Multi-Sensor Camera shall realize SSL / TLS communication with CA certificate. 

15.	A user shall be able to view video on a PC using a browser.

16.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

17.	The Multi-Sensor Camera shall offer Video Motion Detection (VMD) with four (4) per camera programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

18.	The Multi-Sensor Camera shall have Fog compensation function.

19.	The Multi-Sensor Camera shall have High light compensation (HLC) function.

20.	The Multi-Sensor Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

21.	The Multi-Sensor Camera shall provide up to eight (8) areas of electronic privacy masking per camera. 

22.	The multi-sensor camera shall have a USB terminal for confirming the live image and adjusting viewing angle with the smartphone or tablet device via the Wi-Fi connection at installation.

23.	The Multi-Sensor Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

24.	The Multi-Sensor Camera shall have a SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

25.	The Multi-Sensor Camera shall have VMD, and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, and Panasonic alarm protocol output.

26.	The Multi-Sensor Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/3 type CMOS image sensor
2.	Scanning Mode		Progressive
3.	Minimum Illumination
a.	Color		0.09 lux (F2.2, Maximum shutter: Off(1/30s), AGC: 11)
b     B/W                           0.04 lux (F2.2, Maximum shutter: Off(1/30s), AGC: 11)
4.	Day & Night		IR Cut filter Removal
5.	Dynamic Range		108 dB typ. (Super Dynamic: On)

C.	Lens
1.	Vari Focal Length		3.2 mm – 5.7 mm (1/8 inches - 7/32 inches)
2.	Max. Aperture Ratio	1 : 2.2 (WIDE) – 1 : 3.1 (TELE)                                                 
3.	Angular Field of View
a.	16:9 aspect ratio	H: 53° (TELE) - 99° (WIDE)    
V: 30° (TELE) - 54° (WIDE)    
b.	4:3 aspect ratio	H: 44° (TELE) - 81° (WIDE)     
V: 33° (TELE) - 60° (WIDE)     
c.	Focus adjustment	Focus Assist / Manual

             4.     Adjusting Angle                 
                       a.      Camera 1, 2, 3         Horizontal (PAN) angle : 360 °
Vertical (TILT) angle     : +80 to +°30 °
Azimuth (YAW) angle   : ±50 °
                       b.      Camera 4                 Horizontal (PAN) angle : 360 °
Vertical (TILT) angle     : +80 ° to 0 °(right below) to –15 °
Azimuth (YAW) angle   : ±50 °

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio      1920 x 1080 / 1280 x 720 / 640 x 360 / 320 x 180                                                                          
b.     4:3 aspect ratio       1600 x 1200 / 1280 x 960 / 800 x 600 / 640 x 480 / 320 x 240  
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate, VBR, Frame rate, Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30fps
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1,024 / 1,536 / 2,048 / 3,072 / 
4,096 / 6,144 / 8,192 / 10,240 / 12,288 / 14,336 / 16,384 / 20,480 / 24,576 kbps
d.	Image Quality	
i.	Constant bit rate	Motion priority / Normal / Quality priority
ii.	Frame rate            Motion priority / Normal / Quality priority
iii.	Best effort	Motion priority / Normal / Quality priority
iv.	VBR		10 steps
e.	Transmission type	Unicast, Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
On (Frame rate control)* / On (Advanced)* / On (Low) / On (Mid) / Off 
*On (Frame rate control) and On (Advanced) are only available with H.265.
b.	Auto VIQS     	On / Off

E.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off (Only when Intelligent Auto  is off.)
5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
(Only when Super dynamic and Intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Shutter Speed		1/30 to 1/10000
8.	Day & Night		Off/ On(IR Light Off)/ On(IR Light On)/ Auto1(IR Light Off)/
Auto2(IR Light On)/ Auto3(SCC)
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Privacy Zone		On / Off, Up to 8 zones
12.	Camera Title (OSD)	Up to 20 characters
13.	Digital Zoom		x1, x2, x4

F.	NETWORK
1.	Network Interface		10BASE-T / 100BASE-TX / 1000Base-T, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, FTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, IEEE 802.1X, DiffServ
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, FTP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone, Android mobile terminals

G.	INTERFACE
1.	Monitor Output		USB terminal via Wi-Fi connection
2.	SD memory card slot	1 slot, SD/SDHC/SDXC

H.	ELECTRICAL
1.	Power Source		PoE (DC48V/210mA, Class 0)
2.	Power Consumption	Approx. 10.1W

I.	SAFETY / EMC
1.	Safety			UL (UL60950-1), C-UL (CAN/CSA C22.2 No.60950-1), CE, 
				IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024

J.	MECHANICAL
1.	Dimensions 		ø230 mm × 196 mm (ø9-1/16 inches ×7-23/32 inches)
                                           * When using attachment plate only
2.	Weight			Approx. 2.7kg (6.95 lbs) * When using attachment plate only　
3.	Construction material
a.	Main body		Aluminum die cast
b.	Front cover		Polycarbonate resin(with ClearSight coating)
4.	Finish
a.	Main body		Light gray
b.	Front cover		Clear

K.	ENVIRONMENTAL
1.	Ingress Resistance	IP66, IEC60529 measuring standard compatible, Type 4X(UL50), 
NEMA 4X compliant
2.	Vandal Resistance	Compliant with IEC 62262 IK10
3.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F)
 (Power On range: –20 °C to +60 °C {–4 °F to 140 °F})
4.	Operating Humidity	 10 % ~ 95 % (without condensation)