i-PRO WV-ASF950 FACIAL RECOGNITION SERVER SOFTWARE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 13 VIDEO SURVEILLANCE CONTROL AND MANAGEMENT SYSTEMS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd.

B.	Provide Video Surveillance Products from single source manufacturer 

2.2	i-PRO WV-ASF950 FACIAL RECOGNITION SERVER SOFTWARE
A.	GENERAL CHARACTERISTICS
1.	The Facial Recognition Server Software shall perform high precision with deep learning technology
.
2.	The Facial Recognition Server Software (Ver3.1 or later) shall set registered face detection or unregistered face detection* in a facial recognition server.
*Unregistered face detection setting can be used both of Unregistered Face Detection 
and Registered Face Detection simultaneously.

3.	The Facial Recognition Server Software shall recognize the angled face (up to 45 degrees to the left or right or 30 degrees up or down), changed aging and a face with sunglass.

4.	The Facial Recognition Server Software shall connect up to 20 i-PRO cameras with best shot function to a single server depends on the number of people passing and the retention period of the face image.  

5.	The Facial Recognition Server Software in unregistered face detection setting shall connect up to 10 i-PRO cameras with best shot function to a single server depends on the number of people passing and the retention period of the face image.

6.	The Facial Recognition Server Software shall register up to 30,000 faces by two additional
face registration kits. 

7.	The Facial Recognition Server Software shall be equipped with a face search function 
• Face images that camera detected are stored and it can be searched later.
• By searching the face DB, you can display the result of each cameras in chronological 
order and find movement locus of persons.
• Specify camera or date in detected face images and display the result in the list in 
similarity order.

8.	The Facial Recognition Server Software shall be equipped with a face matching function 
 • When it is matched with registered people alarm of face matching is output in real-time
and display an alarm history in the list.
• The alarm history can be searched by time and date, face image, camera and category.
• Specified screen image can be played back on control monitor with double-clicking on an 
alarm history.
• The alarm history can be exported to HTML file.

9.	The Facial Recognition Server Software shall be equipped with a unregistered face matching function 
 • When it is unmatched with registered people, alarm is output* in real-time and display 
an alarm history in the list.
*.When the "Unregistered face detection function" is used, the time that it takes to issue 
the alarm is several seconds longer than the conventional recognition function.
• The alarm history can be searched by time and date and camera.
• Specified screen image can be played back on control monitor with double-clicking on an 
alarm history.
• Persons who don’t have ID card can be detected with Genetec Security Center Synergis
• The alarm history can be exported to HTML file.

10.	The Facial Recognition Server Software shall be equipped with people counting, age and
gender Statistics function.
• Count people of detected face and evaluate their age and gender
• Display the result on the screen with statistical graph
• The statistical data can be saved as a CSV file for analytical use.

11.	The Facial Recognition Server Software shall be performed face matching at one second in 30,000 registered faces after receiving the face thumbnail to facial recognition server. 

12.	Facial Recognition Server Software in unregistered face detection setting shall be performed detection of unregistered face at three seconds collates with 30,000 registered faces after receiving the face thumbnail to facial recognition server.

13.	The Facial Recognition Server Software shall searches for faces at the fastest three seconds out of five million faces depending to search conditions. 

14.	The Facial Recognition Server Software shall keep up to 10 million face thumbnail in facial recognition server. 

15.	The Facial Recognition Server Software shall be linked with the alarm to number of client PC with management software (WV-ASM300 : 16).
File extension of registered face image for import is BMP, JPG and PNG

B.	SYSTEM REQUIREMENT
（Server/Hardware）
1.	CPU                               Intel® Xeon® or CoreTM i7 series 3.40 GHz or faster (4-core
8-thread or better) 32 GB
2.	Memory                         32 GB or more 
3.	HDD                              1 TB or more
4.	Graphic                         NVIDIA® QUADRO® P5000, NVIDIA® QUADRO® RTX5000
5.	Power supply                600 W or more
6.	OS                                Microsoft® Windows® 10 Professional RS5 (64 bit), Microsoft® 
Windows Server® 2016 Standard Edition*1, 
Microsoft® Windows Server® 2019 Standard Edition
*1　End of life date will be January 11, 2022

（Network Camera for face detection）  
WV-SPN631* / WV-SPN611*1/ WV-SPN531A / WV-SPN311A / WV-SPN310A / WV-SP305 / 
WV-SFV631LT *2/ WV-SC385 *3 / WV-S1132 / WV-S1131 / WV-S1112 / WV-S1111 / 
WV-S2531LTN *2 / WV-S6130  

* The Optional IR-LED (WV-SPN6FRL1) cannot be installed with any of the tested Lenses*4 
*2 Although this is the outdoor model, it can be used as face matching camera for indoor only.
*3 After fixing the angle of view, if you control the camera with PTZ operation, the face 
    Matching function will not work properly. In this case, set the view.
*4Tested lenses :  i-PRO do not guarantee the quality, performance, operation of the following third-party products.
    FUJINON : YV3.3x15SA-SA2, YV3.3x15SR4A-SA2, DV10x8SR4A-SA1, YV10x5HR4A-
SA2
TAMRON : M13VG550, M13VG850IR

（Network Disk Recorder）  
WJ-NV300 Series, WJ-NV200 Series, WJ-ND400 Series, WJ-ND300 Series, WJ-NX400 Series, WJ-NX300 Series, WJ-NX200 Series

（Management Software）
1.    i-PRO Central Management software + Extension software  :  WV-ASM300 + WV-ASE231
2.   The unified security platform from Genetec Inc. :
Genetec Security Center V5.8, V5.9 + WV-ASE231 Ver.3.10 or later
3.   Video Insight VMS Software  :  Video Insight IP Server/VI  MonitorPlus V7.8.1 or later 
+ WV-ASE231
4.   Milestone XProtect Corporate 2019 R2, 2020 R2 + WV-ASE231 Ver.3.10 or later

C.	PRODUCTS LINE-UP
1.	PC Software Package : WV-ASF950, WV-ASF950W
2.	Additional Camera Kit : (1ch) WV-ASFE901, WV-ASFE901W
(4ch) WV-ASFE904, WV-ASFE904W
3.	Additional Face Registration Kit : WV-ASFE951,WV-ASFE951W
4.	Extension Software for WV-ASM300, VI  MonitorPlus, Genetec Security Desk, WV-ASE231
5.	Upgrade Software : WV-ASF950UGW