i-PRO WV-ASV100W VEHICLE SEARCH SERVER SOFTWARE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 13 VIDEO SURVEILLANCE CONTROL AND MANAGEMENT SYSTEMS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Products from single source manufacturer 

2.2	i-PRO WV-ASV100W VEHICLE SEARCH SERVER SOFTWARE
A.	GENERAL CHARACTERISTICS

1.	The Vehicle search server software shall perform high precision with deep learning technology.

2.	The Vehicle search server software shall be recognized the 6 vehicle types(Pickup Truck, Sedan, Van, SUV, Truck, Bus)  and 10 vehicle colors (Green, Blue, Brown, Purple, Yellow, Red, Pink, Black, Silver/Gray, White).

3.	The Vehicle search server software shall be detected 8 inbound/ 8 outbound direction of vehicle. 

4.	The Vehicle search server software shall be equipped to search suspicious vehicles by the information – date/time, location, vehicle type, vehicle color or direction.

5.	The Vehicle search server software shall be equipped to have a function of adjusting the accuracy to change number of result by slide bar.

6.	The Vehicle search server software shall be equipped to integrate with map view to detect the vehicle position and direction.

7.	The Vehicle search server software shall be equipped with thumbnail view function 
• Enable to view maximum 64 vehicles on thumbnail at a page.
• Vehicle image playback with 1 click on a thumbnail of search result list.

8.	The Vehicle search server software shall be equipped to mark candidate of suspicious vehicle and change status by marking color in order to narrow down.

9.	The Vehicle search server software shall be equipped to create a case report on the marked suspicious vehicles to print to paper or output PDF file. 

10.	The Vehicle search server software shall be equipped to save and export operation logs
by CSV file.

11.	Vehicle search server software shall be equipped to support up to 20 channels on one servers and enables to connecting of  up to 10 multi-sensor cameras (To use 2 channels per multi-sensor camera) or 20 single cameras can be connected. 

12.	Vehicle search server software shall be equipped to support up to 200 channels on ten servers and enables to connecting of  up to 100 multi-sensor cameras (To use 2 channels per multi-sensor camera) or 200 single cameras can be connected. 

B.	SYSTEM REQUIREMENT
（Vehicle Search Server）
1.	CPU                              Intel® Xeon® Gold 5118 2.3 GHz (12-core 24-thread) or better, 
CoreTM i7-8700K 3.70 GHz (6-core 12-thread) or better
2.	Memory                         32 GB (16 GB x 2) or more
3.	HDD                              3 TB or more (in the case of 31days)
4.	Graphic                         NVIDIA® Quadro P4000 x 2
5.	Power supply                550 W or more
6.	OS                                Microsoft® Windows® 10 Pro (64 bit) Release Ver.1809, 
Microsoft® Windows Server® 2016 Standard Edition 
7.	Network I/F                   1000 Mbps

（Security Center 5.7 client + WV-ASVC101W）
1.     CPU                              IIntel® CoreTM i7-4770 or better
2.     Memory                         8 GB or more
3.     HDD                              120 GB for OS and Security Center applications
4.     Graphic                         NVIDIA® QUADRO® K620 2 GB video card
5.     OS                                Microsoft® Windows® 8.1 Professional (64bit),
Microsoft® Windows® 10 Professional RS4(64bit) English/French 
6.    Network I/F                   1000 Mbps

（VI MonitorPlus 7.4 + WV-ASVC101W）
1.     CPU                              Intel® CoreTM i7-6700 or better
2.     Memory                        8 GB or more
3.     HDD                             120 GB for OS and Video Insight IP Server applications
4.     Graphic                         NVIDIA® QUADRO® K620 2 GB video card
5.     OS                                Microsoft® Windows® 10 Professional (64bit)
6.    Network I/F                   1000 Mbps 

（Recommended Network Camera for Vehicle Search）  
WV-X8570N / i-PRO Extreme Cameras

C.	PRODUCTS LINE-UP
1.	Vehicle Search Server Software : WV-ASV100W
2.	Client Plug-in Software (Genetec / VideoInsight) : WV-ASVC101W
3.	Additional Camera Kit : (1ch) WV-ASVE104W
(4ch) WV-ASVE101W
4.	Update Software (1 year) : WV-ASVM111W