i-PRO WV-CU980 Ethernet System Controller
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd. 

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-CU980 Ethernet System Controller

A.	GENERAL CHARACTERISTICS
1.	The Ethernet System Controller shall control functions of i-PRO network security cameras and recorders via i-PRO management software WV-ASM300 or Video Insight video management software.

2.	The Ethernet System Controller shall be provided an Ethernet connection can be used even away from a PC and installed in a desired location

3.	The Ethernet System Controller shall be equipped detached 3D joystick controls Pan/Tilt and Zoom of camera, allowing seamless tracking

4.	The Ethernet System Controller shall be equipped 3D joystick controller enables to change moving direction (PAN / TILT) and Calibration of lever position.

5.	The Ethernet System Controller shall layout ergonomic key and angle enables ease of operation where blind touch input. 

6.	The Ethernet System Controller shall be equipped authentication function using ID and password for preventing illegal operations.

7.	6.	The Ethernet System Controller shall be equipped LCD screen to display various setting. 

8.	The Ethernet System Controller shall offer an optional face search function for monitoring using a person’s face. 

B.	FUNCTIONS
1.	Monitoring control
Sequence, group, 1 screen, 4 screens, 9 screens, 16 screens Multiscreen Display
Up to 64 multiscreen 

2.	Camera Control
Focus, Iris, Zoom, Pan, Tilt, Preset, Aux(x2), Wiper

3.	Recorder Control 
REC, PLAY, Pause, Stop, FF, FR, Prev. Record, Next Record, Prev. Image, Next Image, 
Go to Last
 
4.	 Display
LCD (16 characters, 2 lines), Adjustable Brightness and Contrast

C.	Supported Management Software
i-PRO WV-ASM300, Video Insight VMS Software

D.	NETWORK
1.	Network Interface		10BASE-T / 100BASE-TX / RJ-45 connector
2.	IP			IPv4
3.	Supported Protocols          TCP/IP
4.	Max. User access		Up to 16 users

E.	ELECTRICAL
1.	Power Source		DC 12 V 250 mA
2.	Power Consumption	Approx. 3W

F.	SAFETY / EMC
1.	Safety			
WV-CU980                        UL (UL60950-1), c-UL (CSA C22.2 No.60950-1)
WV-CU980/G                    CE, IEC60950-1

2.	EMC 			
WV-CU980                        FCC (Part15 Class A), ICES003 Class A
WV-CU980/G                    EN55032 Class B, EN55024

G.	MECHANICAL
1.	Dimensions 		
Main Unit                           237 (W) x 45 (H) x 173 (D) mm
 {9-11/32 (W) x 1-25/32 (H) x 6-13/16 (D) inches}
Joystick Unit                      113 (W) x 121 (H) x 206 (D) mm
 {4-7/16 (W) x 4-25/32 (H) x 8-1/8 (D) inches}

2.	Weight			Main Unit : 0.84 kg {1.85 lbs}, Joystick Unit : 0.64 kg {1.41 lbs}　

3.	Finish
Main unit, panel                Resin, Black
Joystick unit, base            Resin, Black
Joystick unit, joystick        Resin, Black

H.	ENVIRONMENTAL
1.	Operating Temperature	0 °C to +50 °C {32 °F to +122 °F} 
2.	Operating Humidity	5 % ~ 90 % (without condensation)