i-PRO WV-X1571LN FIXED NETWORK CAMERA WITH AI ENGINE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-X1571LN FIXED NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Fixed Camera shall deliver H.265 stream and H.264 stream. 

2.	The Fixed Camera shall produce a resolution of 3840 x 2160 pixels at up to 30 fps 
with a 16:9 aspect ratio. 

3.	The Fixed Camera shall utilize an approximate 1/1.8 type high sensitivity CMOS image sensor. 

4.	The Fixed Camera shall built-in AI engine to enable analytical applications on network edge.
Built-in AI engine supports the detecting suspicious changes in captured scenes, optimizing the image settings of the camera (based on captured scene analysis) for better image usability, and optimizing video compression through captured scenes to save bandwidth. 

5.	The Fixed camera shall enables to install the optional analytics applications with including developed by third party companies using this camera's SDK.

6.	The Fixed Camera shall feature a 132dB wide dynamic range based on Enhanced Super Dynamic and built-in AI engine and Adaptive Black Stretch technology (ABS). 

7.	The Fixed Camera shall produce a color image with a minimum illumination of 0.09 lux and a monochrome image with 0.05 lux at F1.3, shutter speed of 1/30s and AGC 11. 

8.	The Fixed Camera shall offer a built-in IR illumination to produce a clear monochrome image in zero lux conditions with 40m (131feet) irradiation distance.

9.	The Fixed Camera shall be equipped a special coated cover for increasing the operational utility of outdoor cameras in rain weather.

10.	The Fixed Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

11.	The Fixed Camera shall be equipped with AI intelligent auto mode which is the technology for shooting license plate and person’s face more clearly.

12.	The Fixed Camera shall be equipped with GOP controls including smart facial coding and frame control and it reduce bit rate by controlling the image quality of still areas, moving areas, and faces with AI ​​engine.  

13.	The Fixed Camera shall be equipped with corridor mode enables the capture of a more
vertically-oriented area than the normal format would allow.
                                                                                         
14.	The Fixed Camera shall produce encrypted stream.

15.	The Fixed Camera shall realize SSL / TLS communication with CA certificate. 

16.	The Fixed Camera shall be rated to IK10 vandal resistance.

17.	The Fixed Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress.

18.	A user shall be able to view video on a PC using a browser.

19.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

20.	The Fixed Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

21.	The Fixed Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something or the camera direction is changed to shoot a different subject.

22.	The Fixed Camera shall have Fog compensation function.

23.	The Fixed Camera shall have High light compensation (HLC) function.

24.	The Fixed Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

25.	The Fixed Camera shall provide up to eight (8) areas of electronic privacy masking. 

26.	The Fixed Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

27.	The Fixed Camera shall have a SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

28.	The Fixed Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

29.	The Fixed Camera shall have three (3) alarm sources of terminal input, VMD, and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and  TCP alarm notification output.

30.	The Fixed Camera shall conform to the ONVIF G / M / S / T. 

B.	CAMERA
1.	Image Sensor		1/1.8 type CMOS image sensor
2.	Effective Pixels                  Approx. 8.4 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.09 lux (F1.3, Maximum shutter: Off(1/30s), AGC: 11)
b.	B/W			0.0 lux (with IR LED on)
0.05 lux (F1.3, Maximum shutter: Off(1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		132 dB typ. (Super Dynamic: On)

7.	Built-in IR illumination
a.	Irradiation distance	Approx. 40m (131feet)

C.	Lens
1.	Vari-Focal Length		4.3 ~ 8.6mm (5/32 ~ 11/32 inches)
2.	Max. Aperture Ratio	1 : 1.5 (WIDE) ~ 1 : 2.4 (TELE)
3.	Angular Field of View
a.	16:9 aspect ratio	H: 53° (TELE) - 104° (WIDE)
V: 30° (TELE) -   56° (WIDE)
4.	Adjusting Angle                 
                                          Horizontal (PAN) angle: ±180°
Vertical    (TILT) angle: 0 ° to 100 °
Azimuth   (YAW) angle: –190 ° to +100°
5.	Focus Adjustment		Motorized
6.	Optical Zoom Ratio           2.0x (Motorized)

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio 
3840x2160, 2560x1440, 1920x1080, 1280x720, 640x360, 320x180 
 
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps (30fps)
                             1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps (25fps)
             *Super Dynamic: On, Level: 30 or more, 15fps

c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 / 20480 / 
25600 / 30720 / 35840 / 40960 / 51200 kbps
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate            Low (Motion priority) / Normal / Fine (Image quality priority）
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority）
iv.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
On (Frame rate control)* / On (Advanced)* / On (Low) / On (Mid) / Off 
*On (Frame rate control) and On (Advanced) are only available with H.265.
b.	Smart Facial Coding  Off / On(AUTO VIQS) / On(Smart Facial Coding)
*Smart Facial Coding is only available with Stream(1)

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 /  64 kbps
b.	Audio Mode		OFF / Mic(Line) input / Audio output / Interactive (Half duplex) /
Interactive (Full duplex)

F.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off   The level can be set in the range of 0 to 8.
 (Only when AI intelligent auto / auto contrast adjust: Off)

5.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
The level can be set in the range of 0 to 31.
(only when Super dynamic / AI Intelligent Auto : Off) 
6.	Shutter Speed		1/10000 to 1/30 s (30fps mode)
                                          1/10000 to 1/25 s (25fps mode)
7.	Day & Night		Off/ On(IR Light Off)/ On(IR Light On)/ 
Auto1(IR Light Off)/Auto2(IR Light On)/ Auto3(SCC)
8.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
9.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
10.	Scene Change Detection(SCD)     
On / Off, 1 area
11.	Privacy Zone		 On / Off, Up to 8 zones
12.	Camera Title (OSD)	 Up to 20 characters
13.	Digital Zoom		 4x

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, RTP, FTP, SMTP, DNS, NTP,
SNMP, DHCPv6, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, SSL/TLS, LLDP, MQTT
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, FTP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ, SSL/TLS, LLDP, MQTT
4.	Max. User access		Up to 14 users(Depends on network conditions)
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

H.	INTERFACE
1.	Monitor Output		VBS : 1.0 V [p-p] / 75 ohm, NTSC / PAL composite, Pin jack
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack
3.	Audio Output		ø3.5 mm stereo mini jack (monaural output) 
4.	External I/O Terminals	ALARM IN 1 (Alarm input 1/ Black & white input/
Auto time adjustment input) (x1)
 ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)
ALARM IN 3 (Alarm input 3/ AUX OUT) (x1)
5.	SD memory card slot	1 slot, SD/SDHC/SDXC

I.	ELECTRICAL
1.	Power Source		DC 12V/930mA
 PoE (IEEE802.3af compliant) Device : DC48 V 240 mA
2.	Power Consumption	Approx. 11.2W (DC 12V), Approx. 11.5W (PoE) (Class 0 device)

J.	SAFETY / EMC
1.	Safety			UL (UL60950-1), C-UL (CAN/CSA C22.2 No.60950-1), CE, 
				IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024

K.	MECHANICAL
1.	Dimensions 		130 mm (W) x 130 mm (H) x 337 mm (L) Without adaptor box
{5-1/8 inches (W) x 5-1/8 inches (H) x 13-9/32 inches (L)} 
2.	Weight			Approx. 1.7 kg (3.75 lbs.)　Without adaptor box
3.	Construction material
a.	Main body		Aluminum die cast and resin
b.	Outer fixing screws   Stemless steel (Corrosion-resistant treatment)
c.	Front cover		Polycarbonate resin (with ClearSight coating),
4.	Finish
a.	Main body		i-PRO white
b.	Front cover		Clear

L.	ENVIRONMENTAL
1.	Ingress Resistance	IP66 (IEC60529), Type 4X (UL50E), NEMA 4X compliant, 
2.	Vandal Resistance	IK10 (IEC 62262)
3.	Wind Resistance                 Up to 40 m/s {approx. 89 mph}
4.	Operating Temperature	-40 °C ~ +50 °C (-40 °F ~ 122 °F, When IR-LED is on)
-40 °C ~ +60 °C (-40 °F ~ 140 °F, When IR-LED is off)
(Power On range : –30 °C to +60 °C {–22 °F to +140 °F})
5.	Operating Humidity	 10 % ~ 100 % (without condensation)

M.	Optional Extension Software
1.	AI Video Motion Detection   WV-XAE200W
2.	AI Privacy Guard     	   WV-XAE201W