i-PRO WV-X4172 360-degree FISHEYE INDOOR NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-X4172 360-degree FISHEYE INDOOR NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The 360-degree Fisheye Camera shall deliver H.265 stream, H.264 stream and JPEG
stream. 

2.	The 360-degree Fisheye Camera shall produce a resolution of 2992×2992 pixels at up to
30 fps with a fisheye mode. 

3.	The 360-degree Fisheye Camera shall produce a resolution of 2560×1440 pixels at up to 30fps with a double panorama mode.

4.	The 360-degree Fisheye Camera shall utilize an approximate 1/2 type high sensitivity MOS image sensor. 

5.	The 360-degree Fisheye Camera shall feature a 84dB wide dynamic range. 

6.	The 360-degree Fisheye Camera shall produce a color image with a minimum illumination of 0.3 lux and a monochrome image with 0.2 lux at F1.9, maximum shutter of 1/30s and AGC 11.

7.	The 360-degree Fisheye Camera shall generate multiple simultaneous video streams of up to two (2) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

8.	The 360-degree Fisheye Camera shall be equipped with intelligent auto mode monitors scene dynamics and motion to adjust key camera settings automatically in real-time reducing distortion such as motion blur on moving objects.

9.	The 360-degree Fisheye Camera shall be equipped with GOP control of bitrate reducing technology which five control modes included frame rate control for longer recording and less storage.                                                                                                                                       

10.	The 360-degree Fisheye Camera shall produce encrypted stream.

11.	The 360-degree Fisheye Camera shall realize SSL / TLS communication with CA certificate. 

12.	A user shall be able to view video on a PC using a browser.

13.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

14.	The 360-degree Fisheye Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

15.	The 360-degree Fisheye Camera shall offer intelligent Video Motion Detection (i-VMD) with eight (8) detection modes as intruder detection, loitering detection, cross line detection, object detection, scene change detection, people counting, heat-map and moving object remover.

16.	The 360-degree Fisheye Camera shall have Fog compensation function.

17.	The 360-degree Fisheye Camera shall have High light compensation (HLC) function.

18.	The 360-degree Fisheye Camera shall provide up to eight (8) areas of electronic privacy masking. 

19.	The 360-degree Fisheye Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

20.	The 360-degree Fisheye Camera shall have a SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

21.	The 360-degree Fisheye Camera shall have VMD and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser and  TCP alarm notification output.

22.	The 360-degree Fisheye Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/2 type MOS image sensor
2.	Effective Pixels                  Approx. 12.4 mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.3 lux (F1.9, Maximum shutter: Off (1/30s), AGC: 11)
b.     B/W                           0.2 lux (F1.9, Maximum shutter: Off (1/30s), AGC: 11)
5.	Day & Night		Electrical
6.	Dynamic Range		84 dB  (Wide Dynamic Range : On)

C.	Lens
1.	Focal Length		1.4mm (1/16 inches)
2.	Max. Aperture Ratio	1 : 1.9
3.	Angular Field of View        	H: 183 °,      V: 183°
4.	Zoom Ratio		Digital zoom x1, x2, x4

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	Fisheye mode(max.30fps / 25fps)   
  2992×2992 / 2192 x 2192 / 1280 x 1280 / 640 x 640 / 320 x 320
b.	Quad PTZ mode(max.30fps / 25fps)  
2560×1920 / 2048×1536 / 1600 x 1200 / 1280 x 960 / 800 x 600 /
VGA / QVGA
                       c.     Double Panorama mode (max.30fps / 25fps)  
2560×1440 / 1920 x 1080 / 1280 x 720 / 640 x 360 / 320 x 180 
3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR, Frame rate / Best effort

b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps (30fps)
                                  1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps (25fps)                                         
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 / 20480 / 
24576 kbps / --FREE ENTRY--
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate            Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push

E.	OPERATION
1.	Wide Dynamic Range	On / Off
The level can be set in the range of 0 to 31.
2.	intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off (Only when intelligent Auto/auto contrast adjust is off.)
5.	Back light compensation
High light compensation	BLC (Back light compensation) / HLC (High light compensation) /
Off 
(Only when Wide Dynamic Range and Intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Maximum shutter		1/10000 to 1/30 s (30fps mode)
                                          1/10000 to 1/25 s (25fps mode)
8.	Day & Night		Off / Auto
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Intelligent Video Motion Detection
8 detection modes (Intruder Detection, Loitering Detection,
Object Detection, Cross Line Detection, Scene Change Detection, 
People Counting, Heat-map, Moving Object Remover.)
12.	Privacy Zone		On / Off, Up to 8 zones
13.	Camera Title (OSD)	Up to 20 characters

F.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, SMTP, DNS, NTP,
SNMP, DHCPv6, RTP, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, LLDP, SRTP, SSL/TLS, SFTP, MQTT
b.    IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP, 
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP, IGMP, ICMP,
ARP, IEEE 802.1X, DiffServ, LLDP, SRTP, SSL/TLS, SFTP, MQTT
              4.     Max. User access		Up to 14 users
5.    Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

G.	INTERFACE
1.	SD memory card slot	1 slot, SD/SDHC/SDXC

H.	ELECTRICAL
1.	Power Source		PoE (DC48V/150mA, Class 0)
2.	Power Consumption	Approx. 7.2W (PoE)

I.	SAFETY / EMC
1.	Safety			UL (UL60950-1), C-UL (CAN/CSA C22.2 No.60950-1), CE, 
				IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024, EN55035 

J.	MECHANICAL
1.	Dimensions(D x H)	ø150 mm × 49.5 mm (H) (ø5-29/32 inches × 1-15/16 inches (H))
2.	Weight			Approx. 400 g (0.88 lbs)
3.	Construction material
a.	Main body		ABS resin
4.	Finish
a.	Main body		i-PRO white

K.	ENVIRONMENTAL
1.	Operating Temperature	 0 °C ~ +40 °C (32 °F ~ 104 °F)
2.	Operating Humidity	 10 % ~ 90 % (without condensation)