i-PRO WV-X8571N MULTI-SENSOR NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd 

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-X8571N MULTI-SENSOR NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Multi-Sensor Camera shall deliver H.265 stream and H.264 stream.

2.	The Multi-Sensor Camera shall utilize an approximate 1/1.8 type high sensitivity CMOS image sensor. 

3.	The Multi-Sensor Camera shall have four 4K image sensors and produce a resolution of 3840 x 2160 pixels at up to 15 fps with a 16:9 aspect ratio. 

4.	The Multi-Sensor Camera shall have the four repositionable lenses with easy adjustment include a wide range tilt angle (+ 80 degrees to 0 degree(right below) to  -15 degrees) mechanism minimizes blind spots. 

5.	The Multi-Sensor Camera shall have Continuous view assistance feature which is automatically adjusts the angle of view of each horizontally aligned camera to reduce the overlap of images from each camera.

6.	The Multi-Sensor Camera shall feature a 120dB wide dynamic range based on Enhanced Super Dynamic and Adaptive Black Stretch technology (ABS). 

7.	The Multi-Sensor Camera shall produce a color image with a minimum illumination of 0.12 lux and a monochrome image with 0.05 lux(F1.6, shutter speed :1/30s, AGC:11). 

8.	The Multi-Sensor Camera shall be equipped with a special coated cover for increasing the operational utility of outdoor cameras in rain weather.

9.	The Multi-Sensor Camera shall generate multiple simultaneous video streams of up to two (2) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams per camera.

10.	The Multi-Sensor Camera shall be equipped with intelligent auto mode, the technology for shooting license plate more clearly.

11.	The Multi-Sensor Camera shall be equipped with GOP control which has five selectable control modes (including frame rate control) for longer recording and less storage.  

12.	The Multi-Sensor Camera shall produce encrypted stream.

13.	The Multi-Sensor Camera shall realize SSL / TLS communication with CA certificate. 

14.	The Multi-Sensor Camera shall be rated to IK10 vandal resistance

15.	The Multi-Sensor Camera shall be rated to IP66 and NEMA 4X standard against water and dust ingress

16.	A user shall be able to view video on a PC using a browser.

17.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

18.	The Multi-Sensor Camera shall offer Video Motion Detection (VMD) with four (4) per camera programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

19.	The Multi-Sensor Camera shall have Fog compensation function.

20.	The Multi-Sensor Camera shall have High light compensation (HLC) function.

21.	The Multi-Sensor Camera shall have Super Chroma Compensation (SCC) which realizes a better color reproducibility in the low illumination.

22.	The Multi-Sensor Camera shall provide up to eight (8) areas of electronic privacy masking per camera. 

23.	The multi-sensor camera shall have a USB terminal for confirming the live image and adjusting viewing angle with the smartphone or tablet device via the Wi-Fi connection at installation. 

24.	The Multi-Sensor Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

25.	The Multi-Sensor Camera shall have a SD memory card slot that supports SD, SDHC and SDXC memory card for local storage. 

26.	The Multi-Sensor Camera shall be equipped with audio input terminal.

27.	The Multi-Sensor Camera shall have three (3) alarm sources of terminal input, VMD, and command alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, and  TCP alarm notification output.

28.	The Multi-Sensor Camera shall conform to the ONVIF standard. 

B.	CAMERA
1.	Image Sensor		1/1.8 type CMOS image sensor
2.	Effective Pixels                  Approx. 8.4mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.12 lux (F1.6, Maximum shutter: Off(1/30s), AGC: 11)
b.     B/W                           0.05 lux (F1.6, Maximum shutter: Off(1/30s), AGC: 11)
5.	Day & Night		IR Cut filter Removal
6.	Dynamic Range		120 dB typ. (Super Dynamic: On)

C.	Lens
1.	Focal Length		4.6mm (3/16 inches)
2.	Max. Aperture Ratio	1 : 1.6
3.	Angular Field of View
a.	16:9 aspect ratio	H: 97°
V: 53°

               4.     Adjusting Angle                 
                       a.      Camera 1, 2, 3         Horizontal (PAN) angle : 360 °
Vertical (TILT) angle     : +80 ° to +30 °
Azimuth (YAW) angle   : ±50 °
                       b.      Camera 4                 Horizontal (PAN) angle : 360 °
Vertical (TILT) angle     : +80 ° to 0 °(right below) to –15 °
Azimuth (YAW) angle   : ±50 °

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG

2.	Image Resolution
a.	16:9 aspect ratio
3840x2160, 2560x1440, 1920x1080, 1280x720, 640x360, 320x180 

3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 fps (15 fps mode)
                                  1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 fps (12.5 fps mode)
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1024 / 1536 / 2048 / 3072 / 
4096 / 6144 / 8192 / 10240 / 12288 / 14336 / 16384 kbps
--FREE ENTRY--
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate           Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
e.	Transmission type	Unicast port(AUTO) / Unicast port(MANUAL) / Multicast
4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull, Push
5.	Smart Coding
a.	GOP(Group of picture) control
On (Frame rate control)* / On (Advanced)* / On (Low) / On (Mid) / Off 
*On (Frame rate control) and On (Advanced) are only available with H.265.
b.	Auto VIQS     	On / Off

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 /  64 kbps
b.	Audio Mode		OFF / Mic(Line) input 

F.	OPERATION
1.	Super Dynamic		On / Off
The level can be set in the range of 0 to 31.
2.	Intelligent Auto 		On / Off
3.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
4.	Fog compensation	On / Off The level can be set in the range of 0 to 8 
(Only when intelligent Auto  is off.)
5.	Back light compensation
High light compensation	BLC (Back light compensation) / HLC (High light compensation) /
Off  
The level can be set in the range of 0 to 31
 (Only when Super dynamic and intelligent Auto is off)
6.	AGC			The level can be set in the range of 0 to 11.
7.	Shutter Speed		1/10000 to 16/30 s (15fps mode)
1/10000 to 16/25 s (12.5fps mode)
8.	Day & Night		Off / On / Auto1 (Normal) / Auto2 (IR Light) / Auto3 (SCC)
9.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
10.	Video Motion Detection	On / Off, 4 areas, Sensitivity:15 steps, Detection size:10 steps
11.	Privacy Zone		On / Off, Up to 8 zones
12.	Camera Title (OSD)	Up to 20 characters
13.	Digital Zoom		x1, x2, x4

G.	NETWORK
1.	Network Interface		10BASE-T / 100BASE-TX / 1000Base-T, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, SMTP, DNS, NTP,
SNMP, DHCPv6, RTP, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, MQTT、LLDP、SSL / TLS
b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, RTSP, RTP, RTP/RTCP,
SMTP, DHCP, DNS, DDNS, NTP, SNMP, UPnP,
IGMP, ICMP, ARP, IEEE 802.1X, DiffServ, MQTT、LLDP、
SSL / TLS
4.	Max. User access		Up to 24 users
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

H.	INTERFACE
1.	Monitor Output		USB terminal via Wi-Fi connection
2.	Microphone input / Line input
				ø3.5 mm stereo mini jack
3.	External I/O Terminals	ALARM IN 1 (Alarm input 1/ Black & white input/
Auto time adjustment input) (x1)
 ALARM IN 2 (Alarm input 2/ ALARM OUT) (x1)
ALARM IN 3 (Alarm input 3/ AUX OUT) (x1)
4.	SD memory card slot	1 slot, SD/SDHC/SDXC

I.	ELECTRICAL
1.	Power Source		DC 12V/1.2A, 
PoE+ (IEEE802.3at compliant): DC 54V 350 mA,
2.	Power Consumption	Approx.15W (DC 12V), Approx. 20W (PoE+) (Class 4 device)

J.	SAFETY / EMC
1.	Safety			UL (UL60950-1), c-UL (CSA C22.2 No.60950-1), CE, IEC60950-1
2.	EMC 			FCC (Part15 Class A), ICES003 Class A, EN55032 Class B, 
				EN55024

K.	MECHANICAL
1.	Dimensions 		ø230 mm × 196 mm (ø9-1/16 inches ×7-23/32 inches)
                                           * When using attachment plate only
2.	Weight			Approx. 2.8kg (6.17 lbs) * When using attachment plate only　
3.	Construction material
a.	Main body		Aluminum die cast
b.	Outer fixing screws   Stemless steel (Corrosion-resistant treatment)
c.	Front cover		Polycarbonate resin(with ClearSight coating) 
4.	Finish
a.	Main body		i-PRO white
b.	Front cover		Clear

L.	ENVIRONMENTAL
1.	Ingress Resistance	IP66 (IEC60529), Type 4X(UL50E), NEMA 4X compliant 
2.	Vandal Resistance	IK10 (IEC 62262)
3.	Wind Resistance               Up to 40 m/s {approx. 89 mph}
4.	Operating Temperature	-40 °C ~ +60 °C (-40 °F ~ 140 °F)
 (Power On range: –20 °C to +60 °C {–4 °F to 140 °F})
5.	Operating Humidity	 10 % ~ 100 % (without condensation)