i-PRO WJ-NX100 NETWORK DISK RECORDER
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 19 DIGITAL VIDEO RECORDERS AND ANALOG RECORDING DEVICES

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WJ-NX100 NETWORK DISK RECORDER

A.	GENERAL CHARACTERISTICS
1.	The Network Disk Recorder (NDR) shall be an all-in-one recording solution for IP video surveillance system of up to 4 network cameras.

2.	The NDR shall store H.264 video data, H.265 video data, and JPEG.

3.	The NDR shall have the capability of up to 192Mbps total throughput. (Recording throughput: 96 Mbps, Output throughput : 96 Mbps)

4.	The NDR shall offer 2TB (Max.4TB) of gross storage capacity

5.	The NDR shall offer VMD search function which can search the moving of the selected specific area.

6.	The NDR shall record two streams per camera.

　　　　　　　　　　　　　　　　　　　　　　　　
7.	The NDR shall offer displaying videos on the main connected to HDMI interface. 
　
8.	The NDR shall offer the operation and configuration functions to the cameras and NDR from the main monitor connected to HDMI interface and mouse. 

9.	The NDR shall store an encrypted stream and shall display encrypted streams/videos by decrypting.

10.	The NDR shall realize optional SSL / TLS communication with CA certificate. 

11.	The NDR shall offer remote and mobile monitoring on a PC, smartphone and tablet.

12.	The NDR shall conform to the ONVIF standard. 

13.	The NDR shall have 4 PoE ports.

B.	NETWORK DISK RECORDER
1.	Inputs			Up to 4 network camera support 
2.	Protocols			i-PRO series Network cameras　
Onvif NVT conformant camera and encoder

C.	FUNCTIONS
1.	Display
a.	Local display		HDMI / 4K (Main monitor),  analog composite video (Sub monitor)

b.	Multiscreen Display	Main monitor: 2, 3, 4
Sub monitor: 1, 4
Camera control:	Pan, Tilt, Zoom, Focus, Brightness, Preset position call and program (up to 256), Auto mode, Click centering, Wheel zoom, Zoom reset, Auto Back Focus, Aux, Wiper (for WV-SUD638)
c.	System Setup　	Setup page in English, French, Italian, Spanish, German, Russian,
Portuguese, Thai, Simplified Chinese, Traditional Chinese, Japanese

2.	Recording
a.	Image format		H.265, H.264, MJPEG
b.	Frame rate		Up to 60ips per stream (Depending on the Camera)
c.	Recording rate          96 Mbps or less
d.	Audio		G.711 for Onvif, G.726 (ADPCM) 32kbps per stream, 
AAC-LC 64kbps
e.	Recording Mode	Schedule, Event, Pre (by priority), Emergency
f.	Alarm Source	2 terminal inputs, 
4 camera alarms ( TCP alarm notification),  
128 command alarms,
g.	Event Action		Alarm recording, e-mail notification, Alarm message, 
Camera positioning, Terminal output,  TCP alarm notification output, Buzzer, Indicator

3.	Search and Playback
a.	Search mode	Date and time (Calendar), Video Motion Detection (VMD),
Playback by designating a timeline, Thumnail
b.	Playback control	Play, Reverse Play, Pause, Stop, Fast Forward, Fast Reverse, 
Previous Record, Next Record, Previous Image, Next Image, Go to Date, Go to Last
c.	De-warping		1 de-warped playback of fisheye view video

4.	Remote and mobile monitoring
a.	Remote monitoring	Web browser: Microsoft Internet Explorer 11
WV-ASM300 i-PRO management software, V4.20 or later
b.	Mobile monitoring	i-PRO Mobile APP software on iOS and Android
c.	Re-encoding		Up to 2 clients
Encoding: H.264
Resolution: 1280x960, 640x480, 320x240

5.	Management
a.	User registration	Up to 32 users
b.	Simultaneous users	16 or less
c.	Authentication	User authentication (ID and Password), Host authentication,
Alteration detection
d.	User level		Administrator and customizable 3-level user authentication
e.	Quick setup		Set-up wizard with Automatic camera detection
f.	Central management	WV-ASM300 i-PRO management software, V4.20 or later

D.	STORAGE
1.	HDD slot
Internal		2 HDD slots
2.	HDD type			2.5 inch SATA HDD, Up to 2xHDDs can be installed.
3.	RAID			RAID1

E.	INTERFACE
1.	Indicator/Button
a.	Indicator		Status indicator: OPERATE, ERROR, ALARM, REC 
HDD1, HDD2
b.	Button		Buzzer stop
2.	Connections
a.	Network		(For PC) 1x 10BASE-T/100BASE-TX/1000BASE-T(RJ45)
(For Cameras) 4x 10BASE-T/100BASE-TX (RJ45)
b.	Video		1x HDMI, 1x BNC
c.	Audio		1x HDMI (shared with HDMI for Video)
d.	Alarm/Control	10pin Terminal block
e.	Mouse		1x mouse connection port USB2.0
f.	Copy port		1x USB 3.0 port
3.	Slots
HDD			2x HDD slots 

F.	ELECTRICAL
1.	Power Source		100-240 V AC, 50/60 Hz (included AC power adapter)
2.	Power Consumption	Approx. 81.6W (DC48V 1.875 A)

G.	MECHANICAL
1.	Dimensions 		280 mm(W) x 44 mm(H) x 212 mm(D)
{11-1/32 inches (W) x 1-23/32 inches (H) x 8-11/32 inches (D)} 
(Excluding rubber feet and projections)
2.	Weight
a.	With 1 HDD		Approx.1.9 kg (4.2 lbs.) 
b.	With 2 HDDs		Approx. 2.0 kg (4.4 lbs.) 

H.	ENVIRONMENTAL
1.	Ambient Operating Temperature
				+5 °C ~ +45 °C (41 °F ~ 113 °F)
2.	Ambient Operating Humidity
				 5 % ~ 90 % (without condensation)

I.	APPROVALS
1.	Safety / EMC Standard	cUL (UL62368-1 3Ed), FCC Part15 ClassA,
CE (EN62368-1, EN55032 Class B, EN55035)

J.	SOFTWARE OPTIONS
1.	WJ-NXF02 / WJ-NXF02W  Additional Business Intelligence Kit:2ch input per license
2.	WJ-NXS04 / WJ-NXS04W Secure optional license for 4 cameras
3.	WJ-NXS01 / WJ-NXS01W Secure optional license for 1 camera