i-PRO AI NON-MASK DETECTION APPLICATION SOFTWARE
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 13 VIDEO SURVEILLANCE CONTROL AND MANAGEMENT SYSTEMS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Products from single source manufacturer 

2.2	I-PRO AI NON-MASK DETECTION APPLICATION SOFTWARE
A.	GENERAL CHARACTERISTICS

1.	The AI Non-Mask Detection application software shall perform high precision with deep learning technology.

2.	The AI Non-Mask Detection application software shall detect people who are not wearing a mask from faces recognized by the AI, and send an alarm.

3.	The AI Non-Mask Detection application software shall recognize the following types of masks:
Color masks, pattern (geometric) masks, fashion masks and various mask shapes (flat type, pleated type, three-dimensional type) 

4.	The AI Non-Mask Detection application software shall detect up to eight people simultaneously.

5.	The AI Non-Mask Detection application software shall detect faces turned 45° to the left or right or tilted 30° up or down.

6.	The AI Non-Mask Detection application software shall detect faces a minimum of 40 pixels wide (FHD model) or 80 pixels wide (4K model).

7.	The AI Non-Mask Detection application software shall detect faces captured indoors.

B.	SYSTEM REQUIREMENT
1.	Supported network cameras
WV-X2571LN / WV-X2551LN / WV-X2271L /WV-X2251L / WV-X1571LN / WV-X1551LN 
WV-S2536LTN / WV-S2536LN / WV-S2536L / WV-S2236L / WV-S2136L / WV-S2136 / 
WV-S1536LTN / WV-S1536L

C.	PRODUCTS LINE-UP
1.	None