i-PRO AI PRIVACY GUARD APPLICATION SOFTWARE FOR 360-DEGREE FISHEYE NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 13 VIDEO SURVEILLANCE CONTROL AND MANAGEMENT SYSTEMS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Products from single source manufacturer 

2.2	I-PRO AI PRIVACY GUARD APPLICATION SOFTWARE FOR 360-DEGREE FISHEYE NETWORK CAMERA
A.	GENERAL CHARACTERISTICS

1.	The AI Privacy Guard application software shall perform high precision with deep learning technology.

2.	The AI Privacy Guard application software shall capture targets according to the results of detection by AI and then pixelate individuals so that they cannot be identified. 

3.	The AI Privacy Guard application software shall pixelate the following target. 
・Human :
Pixelating is carried out on the area of an image which is judged by AI processing
 to be a human.

4.	The AI Privacy Guard application software shall select a stream subject to pixelation and a stream that is not subject to pixelation. 

5.	The AI Privacy Guard application software shall allow the following drawing methods to be selected for processes performed in this software. 
Blurring: Blurring is done for the detected target.
Block: Block is done for the detected target.

6.	The AI Privacy Guard application software shall be capable of simultaneous detection of up to 100 people.

7.	The AI Privacy Guard application software shall be able to perform pixelated streaming at a frame rate of up to 15fps.

8.	The AI Privacy Guard application software shall support the following shooting modes: "Fisheye" (for ceiling-mounted cameras only), "Panorama", "Double Panorama", "Quad PTZ", and "Single PTZ"
　

B.	SYSTEM REQUIREMENT
1.	Supported network cameras
WV-S4576L / WV-S4576LM / WV-S4556L / WV-S4556LM / WV-S4176 / WV-S4156

C.	PRODUCTS LINE-UP
1.	None