i-PRO WV-S71300-F3 MINI BOX NETWORK CAMERA
TECHNICAL SPECIFICATIONS
DIVISION 28 – ELECTRONIC SAFETY AND SECURITY
28 20 00 ELECTRONIC SURVEILLANCE
28 23 00 VIDEO SURVEILLANCE
28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SONSORS

This specification is intended for use by the design/construction professional and any user of i-PRO Security products to assist in developing project specifications for security and video surveillance systems.  

Specifier Notes:  This guide specification incorporates CSI MasterFormatTM 2014 Edition Numbers and Titles.

Notes in Italics, such as this one, are explanatory and intended to guide the design professional/specifier and user in the proper selection and use of materials. This specification should be modified where necessary to accommodate individual project conditions.

PART 1 GENERAL   

1.01	SUMMARY
1.02	WARRANTY

A.	Provide manufacturer's standard warranty. 

PART 2 PRODUCTS

2.1	MANUFACTURERS

A.	i-PRO Sensing Solutions Co., Ltd

B.	Provide Video Surveillance Camera from single source manufacturer 

2.2	i-PRO WV-S71300-F3 FIXED DOME NETWORK CAMERA

A.	GENERAL CHARACTERISTICS
1.	The Mini Box Camera shall deliver H.265 stream and H.264 stream. 

2.	The Mini Box Camera shall produce a resolution of 1920x1080 pixels at up to 30fps with a 16:9 aspect ratio, 1280x960 pixels at up to 30 fps with a 4:3 aspect ratio, and 2048x1536 pixels at up to 15 fps with a 4:3 aspect ratio.

3.	The Mini Box Camera shall utilize an approximate 1/2.8 type high sensitivity CMOS image sensor. 

4.	The Mini Box Camera shall built-in AI engine to enable analytical applications on network edge. Built-in AI engine supports the detecting suspicious changes in captured scenes, optimizing the image settings of the camera (based on captured scene analysis) for better image usability, and optimizing video compression through captured scenes to save bandwidth.

5.	The Mini Box Camera shall enables to install the optional analytics applications with including developed by third party companies using this camera's SDK.

6.	The mini Box Camera shall produce a color image with a minimum illumination of 0.3 lux and a monochrome image with 0.2 lux at F2.0, shutter speed of 1/30s. 

7.	The Mini Box Camera shall generate multiple simultaneous video streams of up to four (4) H.265 (Main profile) or H.264 (High profile) streams and JPEG streams.

8.	The Mini Box Camera shall be equipped with AI intelligent auto mode which is the technology for shooting license plate and person’s face more clearly.

9.	The Mini Box Camera shall be equipped with GOP controls including smart facial coding and frame control and it reduce bit rate by controlling the image quality of still areas, moving areas, and faces with AI engine.   

10.	The Mini Box Camera shall be equipped with corridor mode enables the capture of 
a more vertically-oriented area than the normal format would allow.

11.	The Mini Box Camera shall produce encrypted stream.

12.	The Mini Box Camera shall realize SSL / TLS communication with CA certificate. 

13.	A user shall be able to view video on a PC using a browser.

14.	A user shall be able to view video on a smartphone and tablet using viewer software for iPhone and Android.

15.	The Mini Box Camera shall offer Video Motion Detection (VMD) with four (4) programmable detection areas, 15 steps sensitivity level and 10 steps detection size.

16.	The Mini Box Camera shall offer Scene Change Detection (SCD) is possible to issue an alarm when a camera is covered with something or the camera direction is changed to shoot a different subject.

17.	The Mini Box Camera shall have Fog compensation function.

18.	The Mini Box Camera shall have High light compensation (HLC) function.

19.	The Mini Box Camera shall provide up to eight (8) areas of electronic privacy masking. 

20.	The Mini Box Camera shall offer the prioritized stream control which transmits a video stream to a specified client PC or recorder preferentially. 

21.	The Mini Box Camera shall have a microSD memory card slot that supports microSD, microSDHC and microSDXC memory card for local storage. 

22.	The Mini Box Camera shall offer full-duplex bi-directional audio communication capability between the camera and monitoring site. 

23.	The Fixed Camera shall have f three (3) alarm sources of terminal input, VMD, command alarm, and audio detection alarm that activate the processes such as SDXC/ SDHC/SD memory recording, E-mail notification, HTTP alarm notification, Indication on browser, FTP image transfer and  TCP alarm notification output.

24.	The Mini Box Camera shall conform to the ONVIF G / M / S / T. 

B.	CAMERA
1.	Image Sensor		1/2.8 type CMOS image sensor
2.	Effective Pixels                  Approx. 2mega pixels
3.	Scanning Mode		Progressive
4.	Minimum Illumination
a.	Color		0.21 lux (30IRE, F2.0, 1/30s)
0.3 lux (50IRE, F2.0, 1/30s)
b.	B/W			0.2 lux (50IRE, F2.0, 1/30s)
5.	Color / BW		Auto / Off

C.	Lens
1.	Focal Length		3.2 mm 
2.	Max. Aperture Ratio	1 : 2.0
3.	Angular Field of View
a.	16:9 aspect ratio	H: 81.1° , V: 51.4°
b.	4:3 aspect ratio	H: 60.8° , V: 51.4° 
4.     Focus Range		0.5m to ∞
5.     Optical Zoom Ratio          1x

D.	VIDEO
1.	Compression Format	H.265, H.264, JPEG
2.	Image Resolution
a.	16:9 aspect ratio (30fps, 25fps)
1920x1080, 1280x720, 640x360, 320x180
b.	4:3 aspect ratio (30 fps, 25fps)
1280x960, 640x480, 320x240
c.	4:3 aspect ratio (15 fps, 12.5fps)
2048x1536, 1280x960, 640x480, 320x240

3.	H.265 / H.264
a.	Transmission Mode	Constant bit rate / VBR / Frame rate / Best effort 
b.	Frame Rate		1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 / 60 fps (60fps)
1 / 3 / 5 / 7.5 / 10 / 12 / 15 / 20 / 30 fps (30fps)
1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 / 50 fps (50fps)
1 / 3.1 / 4.2 / 6.25 / 8.3 / 12.5 / 20 / 25 fps (25fps)
c.	Bit Rate/Client	64 / 128 / 256 / 384 / 512 / 768 / 1,024 / 1,536 / 2,048 / 3,072 / 
4,096 / 6,144 / 8,192 / 10,240 / 12,288 / 14,336 / 16,384 / 20,480 / 24,576 kbps
d.	Image Quality	
i.	Constant bit rate	Low (Motion priority) / Normal / Fine (Image quality priority)
ii.	Frame rate            Low (Motion priority) / Normal / Fine (Image quality priority)
iii.	Best effort	Low (Motion priority) / Normal / Fine (Image quality priority)
iv.	VBR		10 steps
e.	Transmission type	Unicast port (AUTO)/ Unicast port (MANUAL)/ Multicast

4.	JPEG
a.	Image quality	10 steps 
b.	Transmission type	Pull(Refresh Interval)/ Push(MJPEG)

5.	Smart Coding
a.	GOP(Group of picture) control
On (Frame rate control)* / On (Advanced)* / On (Low) / On (Mid) / Off 
*On (Frame rate control) and On (Advanced) are only available with H.265.
b.	Smart Facial Coding  Off / On(High) / On(Low)

E.	Audio
a.	Audio Compression	G.726 (ADPCM) 32kbps / 16kbps, G.711 64kbps, 
AAC-LC 128 / 96 /  64 kbps

F.	OPERATION
1.	Intelligent Auto 		On / Off
2.	Adaptive Black Stretch	The level can be set in the range of 0 to 255.
3.	Fog compensation	On / Off 
 (Only when AI intelligent auto / auto contrast adjust: Off)
4.	Black light compensation
High light compensation	BLC (Black light compensation) / HLC (High light compensation) /
Off 
(Only when intelligent Auto : Off)
5.	Shutter Speed		1/10000 to 16/30 s (15fps,30fps mode)
1/10000 to 16/25 s (25fps,12.5fps mode)
6.	Color / BW		Auto / Off
7.	Digital Noise Reduction	The level can be set in the range of 0 to 255.
8.	Video Motion Detection	On / Off, 4 areas available
9.	Scene Change Detection(SCD)	On / Off, 1 area
10.	Privacy Zone		On / Off, Up to 8 zones
11.	Camera Title (OSD)	Up to 40 characters (alphanumeric characters, marks)
12.	Extra Zoom		1.0 - 3.0x (when resolution is 640x360)

G.	NETWORK
1.	Network Interface		10Base-T / 100Base-TX, RJ-45 connector
2.	IP			IPv6, IPv4
3.	Supported Protocols
a.	IPv6			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, SMTP, DNS, NTP, 
SNMPv1/v2/v3,DHCPv6, RTP, MLD, ICMP, ARP, IEEE 802.1X, DiffServ, SFTP, MQTT, LLDP

b.	IPv4			TCP/IP, UDP/IP, HTTP, HTTPS, SSL/TLS, RTSP, 
RTP,RTP/RTCP,SMTP, DHCP, DNS, DDNS, NTP, SNMPv1/v2/v3, UPnP, IGMP,ICMP, ARP, IEEE 802.1X, DiffServ, SRTP, SFTP, MQTT, LLDP
4.	Max. User access		Up to 14 users
5.	Mobile Terminal Compatibility
iPad, iPhone, AndroidTM mobile terminals

H.	INTERFACE
1.	SD memory card slot	1 slot, microSD/microSDHC/microSDXC

I.	ELECTRICAL
1.	Power Source		DC 5V/1.5A, 
PoE (IEEE802.3af compliant) Device : DC48 V 170mA
2.	Power Consumption	Approx. 7.5W (DC 12V), Approx. 8.2W (PoE) (Class 0 device)

J.	SAFETY / EMC
1.	Safety			UL (UL62368-1), CE
2.	EMC 			FCC (Part15 ClassA), ICES-003 ClassA, EN55032 ClassB,
EN55035

K.	Operating Temperature	-10 °C to +40 °C (14 °F to 104 °F)
Power on : 0 °C ~ +40 °C (32 °F to 104 °F )

L.	Operating Humidity		10 % ~ 90 % (without condensation)

M.	MECHANICAL
1.	Dimensions 		102 mm(W) x 48 mm (H) x 21mm(D)
 { 4-1/32 inches (W) × 1-7/8 inches (H) × 13/16 inches (D) }                                           
2.	Weight			Approx. 157 g 
(excluding the mounting base and protective cover)
Approx. 169 g 
(excluding the mounting base, including the protective cover)
Approx. 197 g
 (including mounting base and protective cover)

3.	Construction material
a.	Main body			PC resin, Aluminum die-casting

4.	Finish
a.	Main body			i-PRO white